#!/bin/bash
cp -f /etc/hostapd/hostapd.conf.iiab /etc/hostapd/hostapd.conf
sed -i -e "s/^#denyinterfaces/denyinterfaces/" /etc/dhcpcd.conf
systemctl enable hostapd
systemctl enable dhcpd
systemctl daemon-reload
systemctl restart dhcpcd
systemctl restart networking
systemctl start hostapd
systemctl start dhcpd

# Temporary promiscuous-mode workaround for RPi's WiFi "10SEC disease"
# Disable "promiscuous" on wlan0 when AP (i.e. no WiFi gateway)
# SEE ALSO iiab-hotspot-off + /usr/libexec/iiab-startup.sh
# https://github.com/iiab/iiab/issues/638#issuecomment-355455454
if grep -qi raspbian /etc/*release; then
    ip link set dev wlan0 promisc off
fi

sed -i -e "s/^HOSTAPD_ENABLED.*/HOSTAPD_ENABLED=True/" {{ iiab_env_file }}

echo -e "\nPlease consider rebooting now.\n"
